(footprint "Bottom Block Connector"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -20.78 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "fa49df0b-d18c-4512-9523-57e0b2315dad")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Bottom Block Connector"
		(at 0 -19.28 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "ba1e0610-1238-4776-9acc-3f52fc1ac274")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1f7754c3-0bc9-4893-a63e-67771568052c")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "da409b30-e1f4-4d76-8e59-cb494ec03ae2")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fa75d831-f30a-4afe-9bbe-0671e18ba5ee")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -10.27626 4.399468)
		(end -3.679314 9.610596)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "26876452-1aad-496c-91c1-54c216c1f0fa")
	)
	(fp_rect
		(start -10.242595 -9.65)
		(end -3.75 -4.44204)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "5aadfba4-fca6-4aa2-bc49-d105e305b9be")
	)
	(fp_rect
		(start 3.75 -9.564666)
		(end 10.290258 -4.427982)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "83f74773-f638-4e7c-bd7c-cd82f2e7036d")
	)
	(fp_rect
		(start 3.75 4.350763)
		(end 10.307438 9.607703)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "b01dcf19-0eb6-4d29-aa4e-a7b1143d471c")
	)
	(fp_text user "GND"
		(at -8.5 -3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "28e44a97-a2cd-4fc2-a283-05bcb1154a59")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "SENSE"
		(at 4.5 -3.347092 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "61f94c83-6733-4d41-97e5-cb61a66dc368")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "+5V"
		(at 5 4.545433 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "7e61648c-d99a-4e13-8b97-ac3853af5633")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "DIN"
		(at -8 4.752044 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "adeee4b3-d76d-4419-a3e0-16a24b919636")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -17.78 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "bfeb8936-2605-46ae-99c2-f611443a4579")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -7 -7)
		(size 4 4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "67f10c74-799d-45f0-9caf-f7788f5f662e")
	)
	(pad "1" smd rect
		(at -7 -7)
		(size 4 4)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "101e8ad9-224f-46b3-87f4-ad0e56bc0bc4")
	)
	(pad "2" smd rect
		(at 7 -7)
		(size 4 4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "a5b1f81b-cb2b-416c-b453-ea4304670bb1")
	)
	(pad "2" smd rect
		(at 7 -7)
		(size 4 4)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "06364b91-e27a-453c-825d-4c93c7f54252")
	)
	(pad "3" smd rect
		(at -7 7)
		(size 4 4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "da72c725-260f-4450-853e-3474c2ff991f")
	)
	(pad "3" smd rect
		(at -7 7)
		(size 4 4)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "0697be5b-a96c-486b-a801-75d3591a3309")
	)
	(pad "4" smd rect
		(at 7 7)
		(size 4 4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "53b0381f-8039-47a9-b28f-377cffe7060a")
	)
	(pad "4" smd rect
		(at 7 7)
		(size 4 4)
		(layers "B.Cu" "B.Paste" "B.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "da7ec61f-94ae-47b7-b5fb-1e456a9d5374")
	)
	(pad "5" thru_hole oval
		(at -9.65 -7)
		(size 1.05 4)
		(drill oval 1 5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "060b8b3e-fa15-49b4-8d73-14375c0ad64d")
	)
	(pad "5" thru_hole oval
		(at -9.65 7)
		(size 1.05 4)
		(drill oval 1 5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "8657d410-6933-4ef5-8bc6-dad62152a522")
	)
	(pad "5" thru_hole oval
		(at -4.35 -7)
		(size 1.05 4)
		(drill oval 1 5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "7ba24e8b-3606-431c-90c0-b5288e924826")
	)
	(pad "5" thru_hole oval
		(at -4.35 7)
		(size 1.05 4)
		(drill oval 1 5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "bf5ae15e-77f9-41b2-b4a1-11208440dc69")
	)
	(pad "5" thru_hole oval
		(at 4.35 -7)
		(size 1.05 4)
		(drill oval 1 5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "58c148af-646d-410d-8f4b-e2c155e36e89")
	)
	(pad "5" thru_hole oval
		(at 4.35 7)
		(size 1.05 4)
		(drill oval 1 5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "52bdcb57-2483-42a3-b7ed-90b871e5022d")
	)
	(pad "5" thru_hole oval
		(at 9.65 -7)
		(size 1.05 4)
		(drill oval 1 5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "b580ebb5-5d3c-468c-915f-dab729108be2")
	)
	(pad "5" thru_hole oval
		(at 9.65 7)
		(size 1.05 4)
		(drill oval 1 5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 45)
		(uuid "3931fdca-ef11-473c-98f8-cf6439321437")
	)
)