(footprint "XL-1615RGBC-WS2812B" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at 0 -12.7 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 1cc34f35-467d-48b2-b5a7-97fe61aa7aed)
  )
  (fp_text value "XL-1615RGBC-WS2812B" (at 0 -11.2 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6be87cd0-00f5-4446-85cd-8570400250b6)
  )
  (fp_text user "${REFERENCE}" (at 0 -9.7 unlocked) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 831430c3-a7d9-4cba-b68b-8926bf5c1176)
  )
  (fp_line (start -0.8 -0.85) (end 0.8 -0.85)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp e0ed9aac-88bf-4fea-9fd3-008546fcf5b1))
  (fp_line (start -0.8 -0.07) (end -0.8 0.07)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 6208798a-0569-445c-b1ba-7d5c66b0d1e8))
  (fp_line (start -0.8 0.85) (end 0.8 0.85)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp 59820e28-c7ea-4011-a69c-9c11511b75b3))
  (fp_line (start 0.8 -0.07) (end 0.8 0.07)
    (stroke (width 0.1) (type default)) (layer "F.SilkS") (tstamp c37cd534-8dc2-475e-bb84-4d1556dc7032))
  (fp_poly
    (pts
      (xy -0.282535 -0.017658)
      (xy 0.005886 -0.22956)
      (xy 0.005886 0.217788)
    )

    (stroke (width 0.1) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 0be5f571-678c-4658-9678-257ddbe063b1))
  (pad "1" smd rect (at -0.75 -0.45) (size 0.8 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 763cdd37-22cc-4626-bf91-dca80ff2d9e3))
  (pad "2" smd rect (at 0.75 -0.45) (size 0.8 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp f7aa557d-2994-4dc7-b37b-75f842414428))
  (pad "3" smd rect (at -0.75 0.45) (size 0.8 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 118bd5f1-9fb9-4bd5-822d-6816257701a9))
  (pad "4" smd rect (at 0.75 0.45) (size 0.8 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45) (tstamp 14e0004c-bdcc-4e07-9796-ab52b0e5cf96))
)
