(footprint "USB_C-0015IPX6-00"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "USB Type C Receptacle, GCT, power-only, 6P, top mounted, horizontal, 3A, 1.9mm stake: https://gct.co/files/drawings/usb4125.pdf")
	(tags "USB C Type-C receptacle power-only charging-only 6P 6C right angled")
	(property "Reference" "REF**"
		(at 0 -5.1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "95c2ba4d-6f60-4594-9ea9-52fbf5601365")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "USB_C-0015IPX6-00"
		(at 0 4.725 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "36f32ef8-742f-42a9-978b-4071d547df0a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "48452a1e-b6b6-483b-a480-2e5b426c1f66")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "831d5ba0-7b98-47b7-b119-a23e98ef81b5")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a7f3feb9-aa8e-4769-9084-30fd557400fa")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5 -3)
		(end -5 -2)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2467febb-d5ab-4f13-ba78-1f2459adc73d")
	)
	(fp_line
		(start -5 0.5)
		(end -5 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "04917f94-e61a-4c18-8712-ddba3eb18db4")
	)
	(fp_line
		(start -5 3.5)
		(end -5 4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a13a0b5e-d319-4f8a-9f2d-efa23569d340")
	)
	(fp_line
		(start -5 4)
		(end 5 4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3104cbec-4990-4bc9-bcab-58b8f648253c")
	)
	(fp_line
		(start -4 4)
		(end -4 5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "2a416804-d4a5-4c93-a467-e64b6cb63e47")
	)
	(fp_line
		(start -4 5)
		(end 4 5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "7adc40c1-0ae8-40f3-93bd-a365cd792d77")
	)
	(fp_line
		(start -3.5 -3)
		(end -5 -3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0793ac5b-0e39-4bac-9727-2273bdad68bc")
	)
	(fp_line
		(start 4 5)
		(end 4 4)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "57cb3702-2187-497d-907a-9c9b2b7bd109")
	)
	(fp_line
		(start 5 -3)
		(end 3.5 -3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "3398e8c7-f41e-4b88-888a-b136675d4e20")
	)
	(fp_line
		(start 5 -2)
		(end 5 -3)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e2517eca-c269-4917-8e4a-5166d1603332")
	)
	(fp_line
		(start 5 1)
		(end 5 0.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "d7b9862c-993d-46c0-ad4e-538c7a8f2d66")
	)
	(fp_line
		(start 5 4)
		(end 5 3.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f88237bc-d487-4689-b306-2a2931b6ffdc")
	)
	(fp_rect
		(start -5.5 -3.5)
		(end 5.5 5.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "dda2e047-5cdf-4070-be01-062d2e931eaf")
	)
	(pad "" np_thru_hole circle
		(at -3.241 -0.523 90)
		(size 1 1)
		(drill 1.05)
		(layers "F&B.Cu")
		(clearance 0.001)
		(uuid "c373b8be-eb90-4ce5-984f-b8b1394e4995")
	)
	(pad "" np_thru_hole circle
		(at 3.258 -0.523 90)
		(size 1 1)
		(drill 1.05)
		(layers "F&B.Cu")
		(clearance 0.001)
		(uuid "ae958a68-ee80-42f0-b00b-a52a9db0d9a8")
	)
	(pad "7" thru_hole oval
		(at -4.9 -0.623)
		(size 1.1 2)
		(drill oval 0.6 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "1aac6f43-0bb8-49ea-98c0-65703e932fa2")
	)
	(pad "7" thru_hole oval
		(at -4.9 2.377)
		(size 1.1 2)
		(drill oval 0.6 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "37897aa5-083e-4a3d-bd12-b6005c8b7f8c")
	)
	(pad "7" thru_hole oval
		(at 4.9 -0.623)
		(size 1.1 2)
		(drill oval 0.6 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "7fde82e7-ab02-4666-a527-4b2a1817dc0b")
	)
	(pad "7" thru_hole oval
		(at 4.9 2.378)
		(size 1.1 2)
		(drill oval 0.6 1.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "2c2d820c-2239-4091-8155-2cf15f14a17a")
	)
	(pad "A5" smd rect
		(at -0.491 -2.378 90)
		(size 1.65 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "5b7cd6fb-d260-4792-892d-e6503b08a70f")
	)
	(pad "A9" smd rect
		(at 1.509 -2.378 90)
		(size 1.65 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "266ca991-f73c-49b1-b44d-00b5f93990c5")
	)
	(pad "A12" smd rect
		(at 2.75 -2.378 90)
		(size 1.65 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "75605fe6-1dcb-45f1-956c-0be2c3154e56")
	)
	(pad "B5" smd rect
		(at 0.509 -2.378 90)
		(size 1.65 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "1d7d450f-ccbb-44f8-b6bb-d1dc6eabafff")
	)
	(pad "B9" smd rect
		(at -1.491 -2.378 90)
		(size 1.65 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "f6f59208-cd25-461c-9a35-79341aa13e6c")
	)
	(pad "B12" smd rect
		(at -2.75 -2.378 90)
		(size 1.65 0.8)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(clearance 0.001)
		(thermal_bridge_angle 45)
		(uuid "6354e3b0-f7fb-44ed-b9cd-9a64f3a9a374")
	)
	(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4125-xx-x-0190_6P_TopMnt_Horizontal.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)