
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "UJC-HP-3-SMT-TR" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -7.62 8.89 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "UJC-HP-3-SMT-TR" (id 1) (at -7.62 -11.43 0)
      (effects (font (size 1.27 1.27)) (justify top left))
    )
    (property "Footprint" "UJC-HP-3-SMT-TR:CUI_UJC-HP-3-SMT-TR" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "CUI Devices" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.16mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "Package" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/UJC-HP-3-SMT-TR/CUI+Devices/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "04/30/2020" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/UJC-HP-3-SMT-TR/CUI+Devices/view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "UJC-HP-3-SMT-TR" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=4722774&manufacturer=CUI Devices&part_name=UJC-HP-3-SMT-TR&search_term=usb c" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "Type C, 20 Vdc, 3 A, Right Angle, Surface Mount, Black Insulator, Power-Only USB Receptacle" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "CUI_purchase_URL" "https://www.cuidevices.com/product/interconnect/connectors/usb-connectors/ujc-hp-3-smt-tr?utm_source=snapeda.com&utm_medium=referral&utm_campaign=snapedaBOM" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 16) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "CUI Devices" (id 17) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "UJC-HP-3-SMT-TR_0_0"
      (rectangle (start -7.62 -10.16) (end 7.62 7.62)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin bidirectional line (at -12.7 5.08 0) (length 5.08)
        (name "CC1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -12.7 2.54 0) (length 5.08)
        (name "CC2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -12.7 0.0 0) (length 5.08)
        (name "V-BUS"
          (effects (font (size 1.016 1.016)))
        )
        (number "A9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -12.7 0.0 0) (length 5.08)
        (name "V-BUS"
          (effects (font (size 1.016 1.016)))
        )
        (number "B9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -12.7 -2.54 0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "A12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -12.7 -2.54 0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "B12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -12.7 -7.62 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -12.7 -7.62 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -12.7 -7.62 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -12.7 -7.62 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "S4"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)