(footprint "Top Block Connector"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -15.24 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "e17cc5d5-dfe8-4b7c-b3a4-be94e94fcbb6")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "Top Block Connector"
		(at 0 -13.74 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4cfe916b-8b6d-4956-b041-31da01915788")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b1f4a813-7f3f-466e-9e58-908afa98f313")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "90c9e94a-3962-4774-bed2-69f37effcfad")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "fbe17dc0-816a-4054-9d0f-378593d7ea01")
		(effects
			(font
				(size 1.27 1.27)
			)
		)
	)
	(attr through_hole)
	(fp_rect
		(start -25 -25)
		(end 25 25)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "02d89982-2879-49da-992f-c4d987f0fd39")
	)
	(fp_rect
		(start -9.044238 -9.06015)
		(end 9.076061 9.048037)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill none)
		(layer "F.CrtYd")
		(uuid "d9ab0ef7-1407-4bc4-abba-b68eb0549242")
	)
	(fp_text user "+5V"
		(at -9 5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0fefd787-ac44-4dd8-80f5-55865fa18581")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "GND"
		(at 5.5 -3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "2c5437a9-0d9d-41e2-8b42-7c4e1c9d7810")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "DOUT"
		(at 5 4.869823 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "41c5b424-fdbd-4dff-86cd-70ab2ec756bb")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "SENSE"
		(at -9.5 -3.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "94cbbe95-193a-4977-9974-403aeb880dff")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left bottom)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 0 -12.24 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "da8bc0ee-d0b9-42f3-a60b-7849c17eba14")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at 7 -7)
		(size 4 4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "94a1ad47-6c3e-4acd-bb59-8651a160cd1e")
	)
	(pad "2" smd rect
		(at -7 -7)
		(size 4 4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "fc4230ad-d73f-42c7-a2e5-c77ff242b0a7")
	)
	(pad "3" smd rect
		(at 7 7)
		(size 4 4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "087c465a-b29c-48e0-aa73-2cdb236c23b3")
	)
	(pad "4" smd rect
		(at -7 7)
		(size 4 4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "ced72edf-782b-4880-9519-3ecdfcb50fb9")
	)
)